TChnCan1.Init  Entry
TChnCan1.Init  Exit
TChnCan1.Done  Entry
TChnCan1.ChClose Entry  SJA=0
TChnCan1.ChClose Exit  SJA=0
TChnCan1.Done  Exit
Wil: Init
TChnCan1.Init  Entry
TChnCan1.Init  Exit
Wil: ChSetParam=NAM=CAN1 ADD=$0300 IRQ=0 BTR=500 SJA=0 CIS=0 LRB=20 LTB=5
Wil: ChResult=$0000
Wil: ChOpen
TChnCan1.ChOpen Entry SJA=0
TestSCN100=1
0 RegWrite: Port[$0309]:=$08 Port[$0301]:=$A0
0 RegRead : Port[$0309]:=$08 Port[$0301] =$A0
TestSJA1000=1
sja_AMode Set ResetMode & AcceptanceFilterMode
0 RegWrite: Port[$0309]:=$00 Port[$0300]:=$01
sja_AClockDivider Set PeliCAN Mode & Bypass input comparator
0 RegWrite: Port[$0309]:=$18 Port[$0307]:=$C0
sja_AOutCtrl HW pouziti vystupu
0 RegWrite: Port[$0309]:=$08 Port[$0300]:=$0A
sja_ABusTiming0
0 RegWrite: Port[$0309]:=$00 Port[$0306]:=$80
sja_ABusTiming1
0 RegWrite: Port[$0309]:=$00 Port[$0307]:=$EF
sja_AcceptCode0 & AcceptMask0
0 RegWriteL:Port[$0309]:=$00 Port[$0308]:=$90 Port[$0300]:=$00000000
0 RegWriteL:Port[$0309]:=$00 Port[$0308]:=$94 Port[$0300]:=$FFFFFFFF
0 RegWrite: Port[$0309]:=$08 Port[$0305]:=$60
sja_RxErrCnt & sja_TxErrCnt
0 RegWrite: Port[$0309]:=$08 Port[$0306]:=$00
0 RegWrite: Port[$0309]:=$08 Port[$0307]:=$00
sja_AMode Set Operating Mode
0 RegRead : Port[$0309]:=$00 Port[$0300] =$01
0 RegWrite: Port[$0309]:=$00 Port[$0300]:=$00
0 RegRead : Port[$0309]:=$00 Port[$0300] =$00
sja_ACmd ClearDataOverrun|ReleaseRecBuff|AbortTransmission
0 RegWrite: Port[$0309]:=$00 Port[$0304]:=$00
0 RegWrite: Port[$0309]:=$00 Port[$0301]:=$0E
0 RegRead : Port[$0309]:=$00 Port[$0303] =$00
TChnCan1.ChOpen Exit  SJA=0
Wil: ChResult=$0000
Wil: ChReceiveBuffer
Wil: ChReceiveResult=$0000
Wil: ChConnect
TChnCan1.ChConnect Entry
TChnCan1.ChConnect Exit
Wil: ChResult=$0000
Wil: ChDisConnect
TChnCan1.ChDisConnect Entry
0 RegWrite: Port[$0309]:=$00 Port[$0304]:=$00
TChnCan1.ChSendFlush - Ok
0 RegWrite: Port[$0309]:=$00 Port[$0301]:=$02
TChnCan1.ChDisConnect Exit
Wil: ChClose
TChnCan1.ChClose Entry  SJA=0
0 RegWrite: Port[$0309]:=$00 Port[$0304]:=$00
0 RegWrite: Port[$0309]:=$00 Port[$0300]:=$01
0 RegWrite: Port[$0309]:=$00 Port[$0300]:=$03
TChnCan1.ChClose Exit  SJA=0
Wil: Done
TChnCan1.Done  Entry
TChnCan1.ChClose Entry  SJA=0
TChnCan1.ChClose Exit  SJA=0
TChnCan1.Done  Exit
Wil: Init
TChnCan1.Init  Entry
TChnCan1.Init  Exit
Wil: ChSetParam=NAM=CAN1 ADD=$0300 IRQ=0 BTR=500 SJA=0 CIS=0 LRB=20 LTB=5
Wil: ChResult=$0000
Wil: ChOpen
TChnCan1.ChOpen Entry SJA=0
TestSCN100=1
0 RegWrite: Port[$0309]:=$08 Port[$0301]:=$A0
0 RegRead : Port[$0309]:=$08 Port[$0301] =$A0
TestSJA1000=1
sja_AMode Set ResetMode & AcceptanceFilterMode
0 RegWrite: Port[$0309]:=$00 Port[$0300]:=$01
sja_AClockDivider Set PeliCAN Mode & Bypass input comparator
0 RegWrite: Port[$0309]:=$18 Port[$0307]:=$C0
sja_AOutCtrl HW pouziti vystupu
0 RegWrite: Port[$0309]:=$08 Port[$0300]:=$0A
sja_ABusTiming0
0 RegWrite: Port[$0309]:=$00 Port[$0306]:=$80
sja_ABusTiming1
0 RegWrite: Port[$0309]:=$00 Port[$0307]:=$EF
sja_AcceptCode0 & AcceptMask0
0 RegWriteL:Port[$0309]:=$00 Port[$0308]:=$90 Port[$0300]:=$00000000
0 RegWriteL:Port[$0309]:=$00 Port[$0308]:=$94 Port[$0300]:=$FFFFFFFF
0 RegWrite: Port[$0309]:=$08 Port[$0305]:=$60
sja_RxErrCnt & sja_TxErrCnt
0 RegWrite: Port[$0309]:=$08 Port[$0306]:=$00
0 RegWrite: Port[$0309]:=$08 Port[$0307]:=$00
sja_AMode Set Operating Mode
0 RegRead : Port[$0309]:=$00 Port[$0300] =$01
0 RegWrite: Port[$0309]:=$00 Port[$0300]:=$00
0 RegRead : Port[$0309]:=$00 Port[$0300] =$00
sja_ACmd ClearDataOverrun|ReleaseRecBuff|AbortTransmission
0 RegWrite: Port[$0309]:=$00 Port[$0304]:=$00
0 RegWrite: Port[$0309]:=$00 Port[$0301]:=$0E
0 RegRead : Port[$0309]:=$00 Port[$0303] =$00
TChnCan1.ChOpen Exit  SJA=0
Wil: ChResult=$0000
Wil: ChReceiveBuffer
Wil: ChReceiveResult=$0000
Wil: ChConnect
TChnCan1.ChConnect Entry
TChnCan1.ChConnect Exit
Wil: ChResult=$0000
Wil: ChDisConnect
TChnCan1.ChDisConnect Entry
0 RegWrite: Port[$0309]:=$00 Port[$0304]:=$00
TChnCan1.ChSendFlush - Ok
0 RegWrite: Port[$0309]:=$00 Port[$0301]:=$02
TChnCan1.ChDisConnect Exit
Wil: ChClose
TChnCan1.ChClose Entry  SJA=0
0 RegWrite: Port[$0309]:=$00 Port[$0304]:=$00
0 RegWrite: Port[$0309]:=$00 Port[$0300]:=$01
0 RegWrite: Port[$0309]:=$00 Port[$0300]:=$03
TChnCan1.ChClose Exit  SJA=0
Wil: Done
TChnCan1.Done  Entry
TChnCan1.ChClose Entry  SJA=0
TChnCan1.ChClose Exit  SJA=0
TChnCan1.Done  Exit
Wil: Init
TChnCan1.Init  Entry
TChnCan1.Init  Exit
Wil: ChSetParam=NAM=CAN1 ADD=$0300 IRQ=0 BTR=500 SJA=0 CIS=0 LRB=20 LTB=5
Wil: ChResult=$0000
Wil: ChOpen
TChnCan1.ChOpen Entry SJA=0
TestSCN100=1
0 RegWrite: Port[$0309]:=$08 Port[$0301]:=$A0
0 RegRead : Port[$0309]:=$08 Port[$0301] =$A0
TestSJA1000=1
sja_AMode Set ResetMode & AcceptanceFilterMode
0 RegWrite: Port[$0309]:=$00 Port[$0300]:=$01
sja_AClockDivider Set PeliCAN Mode & Bypass input comparator
0 RegWrite: Port[$0309]:=$18 Port[$0307]:=$C0
sja_AOutCtrl HW pouziti vystupu
0 RegWrite: Port[$0309]:=$08 Port[$0300]:=$0A
sja_ABusTiming0
0 RegWrite: Port[$0309]:=$00 Port[$0306]:=$80
sja_ABusTiming1
0 RegWrite: Port[$0309]:=$00 Port[$0307]:=$EF
sja_AcceptCode0 & AcceptMask0
0 RegWriteL:Port[$0309]:=$00 Port[$0308]:=$90 Port[$0300]:=$00000000
0 RegWriteL:Port[$0309]:=$00 Port[$0308]:=$94 Port[$0300]:=$FFFFFFFF
0 RegWrite: Port[$0309]:=$08 Port[$0305]:=$60
sja_RxErrCnt & sja_TxErrCnt
0 RegWrite: Port[$0309]:=$08 Port[$0306]:=$00
0 RegWrite: Port[$0309]:=$08 Port[$0307]:=$00
sja_AMode Set Operating Mode
0 RegRead : Port[$0309]:=$00 Port[$0300] =$01
0 RegWrite: Port[$0309]:=$00 Port[$0300]:=$00
0 RegRead : Port[$0309]:=$00 Port[$0300] =$00
sja_ACmd ClearDataOverrun|ReleaseRecBuff|AbortTransmission
0 RegWrite: Port[$0309]:=$00 Port[$0304]:=$00
0 RegWrite: Port[$0309]:=$00 Port[$0301]:=$0E
0 RegRead : Port[$0309]:=$00 Port[$0303] =$00
TChnCan1.ChOpen Exit  SJA=0
Wil: ChResult=$0000
Wil: ChReceiveBuffer
Wil: ChReceiveResult=$0000
Wil: ChConnect
TChnCan1.ChConnect Entry
TChnCan1.ChConnect Exit
Wil: ChResult=$0000
TChnCan1.ChClose Entry  SJA=0
0 RegWrite: Port[$0309]:=$00 Port[$0304]:=$00
0 RegWrite: Port[$0309]:=$00 Port[$0300]:=$01
0 RegWrite: Port[$0309]:=$00 Port[$0300]:=$03
TChnCan1.ChClose Exit  SJA=0
