
Realtek RTL8110S/RTL8169S Gigalan Test Program Tools Ver 0.9

History:0.9


1.Client Requirement :(program of name:CLIENT.EXE)

  a).Need a external connector with RJ45's pin 1<--> pin 3 , pin 2 <--> pin 6.
                                           pin 4<--> pin 7 , pin 5 <--> pin 8.

  b).You could modify the client.cfg file of content to disable/enable
     which item will be tested or not.


       Test item
       num1000=5000                  ;1000Mbps send counter
       num100=3000                   ;100Mbps send counter
       num10=1000                    ;10Mbps send counter

                                     ;if you want test this item
                                     ;set true else false
                                     ;
       1.PG8169      =true/false     ;programming EEPROM data for Giga LAN
       2.Boot_rom    =true/false     ;will be developing in future
       3.speed1000   =true/false     ;force 1000fullMbps
       4.speed100    =true/false     ;force 100fullMbps
       5.speed10     =true/false     ;force 10fullMbps
       6.debug       =true/false     ;show some counters for debugging mode.


  If all of test items were pass , it will show "ooo " & return 0.
  If one of test item was failed , it will stop and show "xxx" & return 1.












